|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UK Nostalgia Superstock Association -**  **Safety requirements for 2017 season** | | **E.T Range and relevant Safety requirement**  If in doubt, please consult MSA rulebook | | |
| **Safety Item** | **Length of certificate** | **14.99 > 12.00** | **11.99 > 10.00** | **9.99 > 9.00** |
| SFI Flex plate 29.1 | 3 years |  |  | X |
| SFI Flex plate shield 30.1 | 5 years |  |  | X |
| SFI Trans shield 4.1 | 5 years if rigid, 2 years if blanket |  | X (at 10.99) | X |
| SFI Bellhousing 6.1 or 6.3 | 2 years |  | X (or 1/4” steel plate surrounding bellhousing, 360 degrees) | X |
| SFI clutch and flywheel 1.1 or 1.2 | 4 years |  |  | X |
| Prop loop | N/A | X (at 13.99) | X | X |
| Neutral safety switch | N/A | X | X | X |
| Auto trans reverse lockout | N/A | X | X | X |
| Water catch can | N/A | X | X | X |
| SFI (or billet steel) harmonic damper | N/A |  | X (at 10.99) | X |
| 5 point SFI or FIA harness | 2 years if SFI, 5 years if FIA |  | X | X |
| Race suit SFI 3.2A/1 | N/A | X | X |  |
| Race suit SFI 3.2A/5 | N/A |  |  | X |
| Gloves SFI 3.3/1 | N/A |  |  | X (at 135 mph) |
| Helmet | Check Snell No. | X | X | X |
| Neck brace/Hans | Hans: 5 years |  | X (at 10.99) | X |
| Roll hoop 10.0 spec | N/A |  | X |  |
| Roll cage 8.50 spec | N/A |  |  | X |
| SFI spec Roll cage padding | N/A |  | X | X |
| Head protector (headrest) | N/A |  | X | X |
| Window net | N/A |  |  | X |
| Fire system | Check system |  |  |  |
| Battery cut off -  NHRA approved type only | N/A | X (if battery relocated) | X (if battery relocated) | X |
| Tail light | N/A | X | X | X |
| Parachute | N/A |  |  | X (at >149 mph) |

X denotes a required item

N/A: Not Applicable

Red denotes items associated with an auto transmission

Blue denotes items associated with a manual transmission